|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Date** | | | | **Est. Delivery Date** | | |
| **Check Completed By** | | | **Serial Number** | | | |
| **Peripheral Components** | | | | | | |
|  | **Remote Control** | | | | | |
|  | **Primary Key** | | | | | |
|  | **Spare Key** | | | | | |
|  | **Bag Cutter (box cutter with PVC Cap)** | | | | | |
|  | **Canopy Assembly** | | | | | |
|  | **Canopy Covering (Tarp)** | | | | | |
|  | **Canopy Mounting Hardware** | | | | | |
|  | **Ball Bungees (24, which includes 2 extras)** | | | | | |
| **Measurement** | | | | | **Value** | **Unit** |
|  | **Air Flow - Idle (2” hose)** | | | |  | **CFM** |
|  | **Air Flow - Full Speed (2” hose)** | | | |  | **CFM** |
|  | **Charging Voltage - Idle** | | | |  | **Volts** |
|  | **Charging Voltage – Full Speed** | | | |  | **Volts** |
|  | **Hour Meter Connected and Incrementing** | | | |  | **Hours** |
| **Checks** | | | | | | |
|  | **Lights working** | | | | | |
|  | **Grease Axle** | | | | | |
|  | **Check Tire Air Pressure** | | | | | |
|  | **Check Engine Oil** | | | | | |
|  | **Run fuel out of fuel tank and carburetor** | | | | | |
|  | **Check Blower Oil Level** | | | | | |
|  | **Service Decal Installed** | | | | | |
|  | **Safety Label Installed** | | | | | |
|  | **Confirm alternator signal wire connector is connected** | | | | | |
|  | **Apply Graphite Lubrication to Hopper and Airlock** | | | | | |
|  | **Check all wire harness secondary locks are installed (fuse box and connectors)** | | | | | |
|  | **Check that all harness connections are connected and locked** | | | | | |
|  | **Remote control function check (100ft from machine)** | | | | | |
|  | **Check for air leaks** | | | | | |
|  | **Burnish in airlock and blower clutch (40 engagements)** | | | | | |
| **Notes** | |  | | | | |